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SHTM 02-01 Part A.17 - Form A17


Anaesthetic gas scavenging system (AGSS) tests - Form A17
	Healthcare organisation/ facility:
	enter text	Date:
	enter a date	Project ref:
	enter text

System details
	Location: enter text

	Department serve: enter text

	Manufacturer: enter text

	Model reference: enter text

	Pump duty (litres/minute): enter text

	Duplex/ simplex: enter text

	Number of remote switches: enter text

	Remote switch voltage (V): enter text


BS EN ISO 7396-2 tests
	Test
	1
	2
	3
	4
	5
	6
	7
	8

	Single flow rates 
	value
	value
	value
	value
	value
	value
	value
	value

	AGSS outlet point @ 1 kilo Pascal (kPa) (80 litres/min maximum)
	value
	value
	value
	value
	value
	value
	value
	value

	AGSS outlet point @ 2 kPa (50 litres/min minimum)
	value
	value
	value
	value
	value
	value
	value
	value


AGSS pump settings
	Pump pressure: enter text millibar (mbar)

	Pump total flowrate: enter text litres/min

	Pump design flowrate: enter text litres/min


Sign off
This is to certify that the above tests have been carried out:
	Test undertaken by:
	Name:
	enter text	Signature:
	enter text	Date:
	enter a date
	Test witnessed by:
	Name:
	enter text	Signature:
	enter text	Date:
	enter a date
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