[image: Public Services Delivery Scotland][image: ]
SHTM 02-01 Part A.12 - Form A12


Plant performance, operation and siting - Synthetic air systems - Form A12
	Healthcare organisation/ facility:
	enter text	Date:
	enter a date	Project ref:
	enter text

System details
	Location: enter text

	Manufacturer/ model: enter text

	Type: Bulk liquid oxygen and nitrogen supply

	Function: choose an item


Performance, operation and siting checklist
	Item
	Function/ operation
	Pass/ fail
	Comments

	1
	Power supplies provided
	pass/ fail	enter text
	2
	General operation
	pass/ fail	enter text
	3
	Leakage on joints
	pass/ fail	enter text
	4
	Indication - system condition panel
	pass/ fail	enter text
	5
	Central alarm panel
	pass/ fail	enter text
	6
	Safety valve exhaust pipes discharge to a safe location
	pass/ fail	enter text
	7
	Separation distances in compliance with Table 5.2 and British Compressed Gases Association (BCGA) CP36
	pass/ fail	enter text
	8
	Compound and blending station room provided with hazard/ warning signs in accordance with Appendix E of SHTM 02-01 Part A
	pass/ fail	enter text
	9
	Access to and within compound and blending station room acceptable
	pass/ fail	enter text
	10
	Lighting provided
	pass/ fail	enter text
	11
	Plant schematic provided
	pass/ fail	enter text


Sign off
This is to certify that the above tests have been carried out:
	Test undertaken by:
	Name:
	enter text	Signature:
	enter text	Date:
	enter text
	Test witnessed by:
	Name:
	enter text	Signature:
	enter text	Date:
	enter a date
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